**F3**

300Mbps wireless router

|  |
| --- |
| **Hardware** |
| Standard&Protocol | IEEE802.3, IEEE802.3u,IEEE802.3ab |
| Interfaces | 1\*10/100Mbps WAN port3\*10/100Mbps LAN ports |
| Antenna | 3\*5dBi external antennas |
| Button | 1\*RST |
| Power | Input：AC 100-240V~50/60Hz 0.6AOutput：DC 9V0.6A |
| Dimension | 185.6\*118.4\*31.2mm |
| LED Indicator | SYS\*1 |
| **Wireless** |
| Wireless Standard | IEEE 802.11b/g/n 2.4GHz |
| Data Rate | 2.4GHz: Up to 300Mbps |
| Frequency | 2.4GHz |
| Transmission Power | CE:<20dBm |
| Basic Features | WiFi On/Off |
| Wireless Security | WPA/WPA2, WPA-PSK/WPA2-PSK |
| **Software** |
| Internet Connection Type | PPPoE, Dynamic IP, Static IPPPPoE(Russia), PPTP(Russia), L2TP(Russia) |
| Operating Mode | Wireless Router ModeUniversal Repeater ModeWISP ModeAP Mode |
| DHCP Server | DHCP ServerDHCP Client ListDHCP Reservation |
| Virtual Server | Port ForwardingDMZ HostUPnP |
| Security | Client Filter Parental Control(support black list and white list)Remote Web Management |
| Firewall | Forbid UDP flood attackForbid TCP flood attackForbid ICMP attackForbid WAN PING from internet |
| DDNS | no-ip,DynDNS,Oray |
| VPN | IPsec pass throughPPTP pass throughL2TP pass through |
| Special Features | Smart WiFi Schedule |
| Others | Bandwidth ControlMAC CloneSystem LogBackup & Restore configurationsFirmware upgradeable via browserIPv6 Features Supported（just in Bangladesh） |
| **Others** |
| Temperature | Operating Temperature: 0℃ ~ 40℃Storage Temperature: -40℃ ~ 70℃. |
| Humidity | Operating Humidity:10% ~ 90% RH non-condensingStorage Humidity: 5% ~ 90%RH non-condensing. |
| Default Settings | Default Access: 192.168.0.1 |
| Certification | CE/FCC/RoHS |
| EIRP Power (Max) | 2.400-2.4835GHz:19.37dBm (EIRP) |
| Package Contents | Wireles Router\*1Power Adapter \*1Install Guide\*1Ethernet Cable\*1 |