**O1-5G**

5GHz 9dBi 11AC 867Mbps Outdoor CPE

|  |  |
| --- | --- |
| **Product Information** | |
| Model | O1-5G |
| Dimension | 132\*72\*46.3mm |
| Deployment | Pole/Wall Mount |
| Application Scenarios | PtP and PtMP wireless connection for Privated ISP access or CCTV Surveillance |
| **Hardware** | |
| Frequency Range | 5GHz |
| Compliant Standards | IEEE 802.11a/n/ac |
| Maximum Wireless Rate | 867Mbps |
| Interfaces | 1\*10/100Mbps LAN Port |
| Antenna Polarization | Dual Polarization |
| Antennas Gain | 9dBi |
| Antenna Beamwidth | Horizontal: 30° Vertical: 30° Elevation: 30° |
| GND | - |
| Reset Button | 1\*Reset Button |
| Power Consumption | 4.7W |
| Waterproof Level | IP65 |
| LED Indicator | PoE/LAN,LED1,LED2 |
| Power Method | 12V 1A Passive PoE  12V 1A DC |
| Lightning Protection | - |
| Passive PoE | Passive power over ethernet via PoE/LAN (+4,5pins  -7,8pins ) up to 60 meters  Voltage range: 9-13V DC |
| Reception Sensitivity | 11a 6Mbps -92dBm±1.5dBm  11n MCS7 HT20 -72dBm±1.5dBm  11ac MCS9 HT80 -64dBm±1.5dBm |
| **Software** | |
| TDMA | - |
| Operating mode | AP/Station |
| Enable/Disable Wireless Radio | Support |
| SSID Hidden | Support |
| Wireless Client isolation | Support |
| SSID Isolation | - |
| Channel Bandwidth | 20/40/80MHz |
| Channel Shift | Support |
| Client Limitation For SSID | Support |
| Wireless Access Control | Support |
| Weak Signal Client Limitation | - |
| Transmission Power | Adjustable power by 1dBm |
| WMM Capable | Support |
| APSD Capable | Support |
| Wireless Security | 64/128 WEP,WPA-PSK,WPA2-PSK,WPA&WPA2-PSK |
| Transparent Bridge | Support |
| VLAN Tagging for SSID | - |
| DHCP Server | - |
| VPN Pass-Through | PPTP,L2TP |
| Remote Web access | - |
| Schedule Reboot | Support |
| Page Timeout | Support |
| Ping Watchdog | Support |
| Dyndns | - |
| Network Diagnoses | - |
| Time and Date Setting | Support |
| Firmware upgrade | Support |
| Backup/Restore Configuration | Support |
| Username Managerment | Support |
| System Logs | Support |
| Managed By Controller | PC Software -- CPE Assistant |
| **Others** | |
| Package Contents | 1\*5GHz 9dBi 11AC 867Mbps Outdoor CPE  1\*Power Adapter  1\*PoE Injector  1\*Quick Installation Guide |
| Operation Temperature | -30℃ ~ 60℃ |
| Storage Temperature | -40℃ ~ 70℃ |
| Operating Humidity | 10%~90% non-condensing |
| Storage Humidity | 10%~90% non-condensing |
| Default login IP | 192.168.2.1 |
| Default Login Username | admin |
| Default Login Password | admin |
| Certification | FCC/CE/RoHS |