**W311MI v6.0**

AX300 Wi-Fi 6 Wireless Nano USB Adapter

|  |  |
| --- | --- |
| **Hardware** | |
| Interfaces | USB2.0 |
| Antenna Type | Internal Antenna |
| Button | - |
| LED Indicator | - |
| Dimension | 21mm × 15mm × 7.7mm(L x W x H) |
| **Wireless** | |
| Wireless Standard | IEEE802.11b,IEEE 802.11g, IEEE 802.11n,IEEE 802.11ax |
| Frequency | 2.4GHz |
| Data Rate | 2.4GHz: Up to 286Mbps |
| Transmission Power | <20dBm (EIRP)  <0.1W(EIRP) |
| Wireless Modes | Station Mode  SoftAP Mode |
| Wireless Security | WPA-PSK/WPA2-PSK  WPA/WPA2 |
| **Others** | |
| Certification | CE FCC UKCA RoHS |
| Package Contents | 1 \* W311MI Wireless Adapters  1 \* Quick Insatalltaion Guide |
| System Requirements | Windows 7/10/11  Linux 3.2+  UOS |
| Environment | Operating Temperature : 0℃ ~ 45℃  Storage Temperature : -40℃ ~ 70℃  Operating Humility:10% ~ 90%RH Non-condensing  Storage Humility:3% ~ 90%RH Non-condensing |
| Related Products | TX2 Pro,TX12 Pro |